{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":7,"n_cols":8,"rows_kept":7,"merged":[[1,0,1,7],[2,0,2,7],[4,7,5,7],[6,0,6,5]]}
[]
["电动门报价单"]
["单位：南平市第二医院（胃镜器械盥洗室）电动门"]
["序号","名称","规格及参数","单位","数量","单价（元）","金额（元）","参数说明"]
[1,"脚踏感应自动门"," M930*2300","樘",1,null,null,"1、门体材质:厚度40 门体材质为1m被锌钢板喷塑，铝合金框架，颜色支持定制，内部框架结构填充阻燃纸蜂窝,铝合金包边,双面不锈钢防撞腰带。\n2、轨道/盖板材质:高强度铝合金(表面电泳发白处理)。\n3、美观性: 门体盖板附带 LED “手术中”指示灯 ; 门体带400*600双层5mm钢化玻璃观察窗,内外内嵌扣手。\n4、气密性: 门体四边铝合金收边，且穿有EVA灰色密封胶条，有效堵住门体与墙面之间的缝隙，保证密封性。\n5、门框不锈钢门套。"]
[2,"不锈钢门套","80+80+300","m",5.6]
["合计(人民币)"]