{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":7,"n_cols":6,"rows_kept":7,"merged":[[1,0,1,5],[4,5,5,5]]}
[]
["急诊楼楼梯不锈钢扶手安装"]
[]
["序号","项目名称","数量（米）","单价（元）","合计","材料参数及做法"]
[1,"楼梯加装不锈钢扶手（靠墙扶手）",66,null,{"$f":"D5*C5","v":0},"1、扶手面管规格：Φ60*1.2mm，材质：202不锈钢；\n2、支撑管规格：Φ51*1.2mm，材质：202不锈钢；\n3、含：支撑管配202不锈钢材质装饰盖；\n4、中间栏板扶手拆除原木扶手后原位安装，新装扶手面高度1050mm高；\n5、靠墙扶手安装于墙面，扶手面高度1050mm高；"]
[2,"楼梯加装不锈钢扶手（中间栏板扶手）",36,null,{"$f":"D6*C6","v":0}]
[{"$nulls":4},{"$f":"SUM(E5:E6)","v":0},"备注：完成后按实测量，按实结算"]