{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":30,"n_cols":8,"rows_kept":30,"merged":[[0,1,0,7],[1,1,1,7],[3,0,10,0],[3,1,10,1],[3,3,10,3],[3,4,10,4],[3,5,10,5],[3,6,10,6],[3,7,10,7],[11,0,17,0],[11,1,17,1],[11,3,17,3],[11,4,17,4],[11,5,17,5],[11,6,17,6],[11,7,17,7],[18,0,21,0],[18,1,21,1],[18,2,21,2],[18,3,21,3],[18,4,21,4],[18,5,21,5],[18,6,21,6],[18,7,21,7],[22,0,24,0],[22,1,24,1],[25,1,25,7],[27,3,27,4],[28,3,28,4],[29,3,29,4],[29,5,29,7]]}
[null,"医疗废弃物收集设备清单"]
[null,"采购单位：南平市第二医院"]
["序号","型号 \nArticle No.","功能特点\nFeatures","单位","数量","单价（元）","合计（元）","备注"]
[1,"\n电助力封闭式医废车\n\n","尺寸：≥1800mm（长）×≥800mm(宽）×≥1400mm(高）\n","台",1]
[null,null,"车头镀锌板喷塑，车箱都采用304材质不锈钢，底框架采用镀锌管，带医废标识。"]
[null,null,"供电方式：钠离子电池24V40Ah"]
[null,null,"屏幕尺寸：≥10寸工控屏；"]
[null,null,"扫描枪：影像式扫码枪，扫码距离60-250MM，扫描精度≥5mill。"]
[null,null,"储放空间：900L"]
[null,null,"称重：最大500kg，箱体底部四个称重传感器。"]
[null,null,"设备与福建省医疗废弃物监督监测系统对接，数据与亲清实时共享"]
[2,"终端蓝牙台秤\n(HYRS-6529B)","最大秤量范围:100/150公斤(kg)单位:公斤/磅(可选)","台",1]
[null,null,"秤量精度:20/50/100克(g)"]
[null,null,"外观尺寸:450x320x45mm；秤盘尺寸:390x320mm"]
[null,null,"整体重量:2.5公斤(kg)"]
[null,null,"显示:LCD液晶带背光"]
[null,null,"功能:归零和去皮；永不关机/120/180/300秒自动关机"]
[null,null,"设备与福建省医疗废弃物监督监测系统对接，数据与亲清实时共享"]
[3,"二维码塑料封条（耗材）",null,"条",72000]
[]
[]
[]
[4,"定位二维码（耗材）","科室定位二维码：100mm*120mm","张",35,null,null,"每个科室标配使用。"]
[null,null,"废弃物箱、暂存间定位二维码：100mm*120mm","张",3,null,null,"医废暂存间标配使用。"]
[null,null,"医护人员、交接人员二维码：50mm*70mm","张",432,null,null,"每位护士、收集人员标配1张人员交接码，用于医废袋收集交接授权使用。"]
["备注：","1、硬件设备质保12个月（验收合格之日起计）；\n2、设备单价含税、安装、运费等一切费用。"]
[null,"3、报价产品可优于上述功能特点"]
[null,"4、耗材数量为暂估量，按实结算。",null,"报价单位："]
[{"$nulls":3},"联系方式：",null," "]
[{"$nulls":3},"日    期："]