{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":32,"n_cols":8,"rows_kept":32,"merged":[[2,0,3,7],[4,0,4,7],[5,0,5,1],[5,2,5,7],[6,2,6,4],[7,2,7,4],[8,2,8,4],[9,2,9,4],[10,2,10,4],[11,2,11,4],[12,2,12,4],[13,2,13,4],[14,2,14,4],[15,2,15,4],[16,2,16,4],[17,2,17,4],[18,2,18,4],[19,2,19,4],[20,2,20,4],[21,2,21,4],[22,2,22,4],[23,2,23,4],[24,2,24,4],[25,2,25,4],[26,2,26,4],[27,2,27,4],[28,0,28,1],[28,2,28,7],[29,0,29,1],[29,2,29,7],[30,7,30,10],[31,4,31,7],[32,5,32,7]],"flags":["formulas_cached_only"]}
[]
[]
["防雷装置检测报价清单"]
[]
["委托(需方)单位：福建省南平市第二医院—业务用房（内科楼（含负压病房）、DSA、病房综合大楼、门诊楼、急诊科-放射科、体检站（含发热门诊、病理科、中西房仓库）、肾内科、血透室、高压氧仓、PCR、污水处理站、医疗垃圾房、外科大楼门卫房、超市、食堂、水塔、职工之家、行政办公楼、设备科、总务仓库、宿舍楼）"]
["收费依据",null,"    依据闽价服[2015]242号文件规定收费，附件1：第1条、建（构）筑物、危险品、易燃易爆场所和设施防雷、防静电装置定期检测，每个检测点（高度15米以下）80元，检测点高度15米以上每增高5米每个检测点加收5元；第2条、电子信息系统机房防雷、防静电装置定期检测，每平方米（使用面积）80元；第5条、电涌保护器常规测试每只60元。（报价不得高于收费标准）"]
["序号","建（构）筑物   名称","检测内容",null,null,"收费单价  （元）","检测点数","小计金额（元）"]
[1,"内科楼（含负压病房）","接闪带、引下线、接地预留测试点、配电箱接地、设备接地、电梯接地等构件",null,null,"/点 ","≥25"]
[2,"DSA","接闪带、引下线、接地预留测试点、配电箱接地、核磁共振设备接地、CT机接地、碎石机接地、辅助设备接地等构件",null,null,"/点 ","≥32"]
[3,"病房综合大楼","接闪带、引下线、接地预留点、屋面设备（管道）接地、配电箱接地、配电柜接地、发电机房接地、消防设备（箱体）接地、桥架接地、设备接地、钢柱接地、电梯接地等构件",null,null,"/点","≥110"]
[4,"门诊楼","接闪带、引下线、接地预留测试点、配电箱接地、低压配电柜接地、发电机房接地、电梯接地、桥架接地、设备接地、金属屋面接地等构件",null,null,"/点 ","≥65"]
[5,"急诊科-放射科","接闪带、引下线、接地预留测试点、配电箱接地、设备接地等构件",null,null,"/点 ","≥38"]
[6,"体检站（含发热门诊、病理科、中西房仓库）","接闪带、引下线、接地预留测试点、配电箱、设备接地等构件",null,null,"/点 ","≥25"]
[7,"肾内科","接闪带、引下线、接地预留测试点、配电箱接地、设备接地等构件",null,null,"/点 ","≥18"]
[8,"血透室","接闪带、引下线、接地预留测试点、配电箱接地、设备接地等构件",null,null,"/点 ","≥17"]
[9,"PCR","接闪带、引下线、接地预留测试点、配电箱接地、低压配电柜接地、电梯接地、桥架接地、设备接地、金属屋面接地等构件",null,null,"/点 ","≥10"]
[10,"污水处理站","接闪带、引下线、金属棚架接地、配电箱接地、设备接地等",null,null,"/点 ","≥4"]
[11,"医疗垃圾房","金属棚架接地、配电箱接地",null,null,"/点 ","≥4"]
[12,"外科大楼门卫房","金属构架接地、配电箱接地等",null,null,"/点 ","≥2"]
[13,"超市","金属构架接地",null,null,"/点 ","≥2"]
[14,"食堂","金属构架接地、配电箱接地等",null,null,"/点 ","≥3"]
[15,"行政办公楼","配电箱接地设备及辅助设备接地等",null,null,"/点 ","≥40"]
[16,"宿舍楼","接闪带、引下线、金属构架接地、配电箱接地等",null,null,"/点 ","≥10"]
[17,"设备科","金属棚架接地、配电箱接地",null,null,"/点 ","≥5"]
[18,"总务仓库","金属棚架接地、配电箱接地",null,null,"/点 ","≥3"]
[19,"高压氧舱","接闪带、引下线、接地预留测试点、配电箱接地、设备接地等构件",null,null,"/点 ","≥25"]
[20,"院区水塔 ","接闪带、引下线接",null,null,"/点 ","≥4"]
[21,"职工之家","金属构架接地、配电箱接地等",null,null,"/点 ","≥13"]
["合计金额"]
["备注",null,"                                                                                     "]
[]
[{"$nulls":4},"2024-01-08"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}